Economic Commission for Europe

Inland Transport Committee

Working Party on the Transport of Dangerous Goods 16 September 2015

Joint Meeting of the RID Committee of Experts and the
Working Party on the Transport of Dangerous Goods

Geneva, 15–25 September 2015

Item 2 of the provisional agenda

**Harmonization with the United Nations Recommendations**

**on the Transport of Dangerous Goods**

 Amendments to 5.2.2.2.1.3

 Note by the secretariat

5.2.2.2.1.3 At the end of sub-paragraph (c), replace the full stop by a semi-column and insert, below that sub-paragraph, the following:

“except that for model No. 9A, the upper half of the label shall only contain the seven vertical stripes of the symbol and the lower half shall contain the group of batteries of the symbol and the class number.”.

At the beginning of the last paragraph, insert “Except for model No. 9A,”.

*[Replaces the amendments to 5.2.2.2.1.3 (a) and 5.2.2.2.1.5 proposed in ECE/TRANS/WP.15/AC.1/2015/23/Add.1]*

5.2.2.2.1.3 Ajouter le texte suivant après l’alinéa c):

“Toutefois, pour le modèle No 9A, la moitié supérieure de l’étiquette doit contenir les sept lignes verticales du signe conventionnel et la moitié inférieure doit contenir groupe de batteries du signe conventionnel et le numéro de la classe.”.

Au début du dernier paragraphe, ajouter: «Sauf pour le modèle No 9A,»

*[Remplace les amendements au 5.2.2.2.1.3 a) et au 5.2.2.2.1.5 proposés dans le document ECE/TRANS/WP.15/AC.1/2015/23/Add.1]*