Proposal for draft amendments to UN Regulation No. 43 (Safety glazing)

The text reproduced below was prepared by the expert from OICA to remove some inconsistencies between UN GTR No. 6 and UN Regulation No. 43. This document comes in addition to ECE/TRANS/WP.29/GRSG/2017/15.The modifications to the current text of Regulation No. 43 are marked in bold characters for new and strikethrough for deleted characters.

**I. Proposal**

*Annex 21, paragraph 1.3.1.,* amend Table 2 to read:

"Table 2

| *Seat-back angle*  *(in °)* | *Horizontal  co-ordinates*  *X* | *Vertical  co-ordinates*  *Z* | *Seat-back angle*  *(in °)* | *Horizontal co-ordinates*  *X* | *Vertical co-ordinates*  *Z* |
| --- | --- | --- | --- | --- | --- |
| 5  6  7  8  9  10  11  12  13  14  15  16  17  18  19  20  21  22 | - 186 mm  ~~- 176~~ **-177** mm  - 167 mm  - 157 mm  - 147 mm  - 137 mm  - 128 mm  - 118 mm  - 109 mm  - 99 mm  - 90 mm  - 81 mm  ~~- 71~~ **-72**  mm  - 62 mm  - 53 mm  - 44 mm  - 35 mm  - 26 mm | 28 mm  27 mm  27 mm  ~~26~~ **27** mm  26 mm  25 mm  24 mm  23 mm  22 mm  21 mm  20 mm  18 mm  17 mm  15 mm  13 mm  11 mm  9 mm  7 mm | 23  24  25  26  27  28  29  30  31  32  33  34  35  36  37  38  39  40 | - 17 mm  - 9 mm  0 mm  9 mm  17 mm  26 mm  34 mm  43 mm  51 mm  59 mm  67 mm  76 mm  84 mm  92 mm  100 mm  107 mm  115 mm  123 mm | 5 mm  2 mm  0 mm  - 3 mm  - 5 mm  - 8 mm  - 11 mm  - 14 mm  ~~- 17~~ **-18** mm  - 21 mm  - 24 mm  - 28 mm  ~~- 31~~ **-32** mm  - 35 mm  - 39 mm  - 43 mm  - 47 mm  - 52 mm |

"

**II. Justification**

Alignment with the corresponding values in UN GTR No. 6 and UN Regulation No. 125. This document completes ECE/TRANS/WP.29/GRSG/2017/15 and does not supersede it.