**Comment on document ECE/TRANS/WP.29/GRSG/2017/15** - Proposal for Supplement 7 to the 01 series of amendments to Regulation No. 43 (Safety glazing)

(Addition to existing text of ECE/TRANS/WP.29/GRSG/2017/15 is shown in bold italic text and deletion in double strikethrough and highlighting all modifications)

**I. Proposal**

*Annex 21* ***Annex 18****, Table 2,* amend to read:

"

| *Seat-back angle**(in °)* | *Horizontal co-ordinates**X* | *Vertical co-ordinates**Z* | *Seat-back angle**(in °)* | *Horizontalco-ordinates**X* | *Verticalco-ordinates**Z* |
| --- | --- | --- | --- | --- | --- |
| 5678910111213141516171819202122 | - 186 mm ***- 177 mm*** - 176mm- 167 mm- 157 mm- 147 mm- 137 mm- 128 mm- 118 mm- 109 mm- 99 mm- 90 mm- 81 mm ***- 72 mm*** - 71 mm- 62 mm- 53 mm- 44 mm- 35 mm- 26 mm | 28 mm27 mm27 mm ***27 mm*** 26 mm26 mm25 mm24 mm23 mm22 mm21 mm20 mm18 mm17 mm15 mm13 mm11 mm 9 mm 7 mm | 232425262728293031323334353637383940 | - ~~17~~ **18** mm- 9 mm0 mm9 mm17 mm26 mm34 mm43 mm51 mm59 mm67 mm76 mm84 mm92 mm100 mm~~107~~ **108** mm115 mm123 mm |  5 mm ~~2~~ **3** mm 0 mm- 3 mm- 5 mm- 8 mm- 11 mm- 14 mm- 17 mm- 21 mm- 24 mm- 28 mm- 31 mm- 35 mm- 39 mm- 43 mm- ~~47~~ **48** mm- 52 mm |

"

**II. Justification for comments**

When proposal is compared with corresponding Table 2 of UN GTR No. 6, highlighted mismatch were found.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_