|  |  |  |
| --- | --- | --- |
|  |  | **INF.40** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods**

Bern, 12-16 March 2018 **8 March 2018**

Item 2 of the provisional agenda

**Tanks**

Correction in the Table in 6.8.2.6.1

Transmitted by the Government of France

1**.** In the Table in 6.8.2.6.1 of RID/ADR, under “For equipment”, the following Note appears under the title of standards EN 14432 and EN 14433:

***“NOTE:*** *This standard may also be used for tanks with a maximum working pressure not exceeding 0.5 bar.”*

2**.** This Note should be amended to take into account the new wording “gravity-discharge tanks”.

Proposal

**6.8.2.6.1** Amend the Table, under “For equipment”, as follows:

– Under the title of standards EN 14432:2014 and EN 14432:2014, in the Note, replace “*tanks with a maximum working pressure not exceeding 0.5 bar”* by *“gravity-discharge tanks*”.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_