Proposal for corrections to UN Regulation 65 (Special Warning Lamps) based upon Supplement 10 to the original Regulation

A recent review of the content of UN Regulation 65 has revealed some long-standing editorial errors that do not affect the technical requirements but do create confusion.

The proposals for the corrections to the existing text of the Regulation are marked in bold for new or strikethrough for deleted characters.

*Paragraph 1.3.,* correct to read:

“1.3. The frequency f is the number of flashes or groups of flashes (see Annex 5, para. ~~5~~**6**) within one second,”

*Paragraph 2.2.5.,* correct to read:

“2.2.5. Two samples, in principle for a rated voltage of 12 volts and for only one colour, and eventually two other samples for any other rated voltage in the case where an application is submitted simultaneously or subsequently for approval of special warning lamps of other rated voltages. In this case, it is sufficient to carry out tests according to paragraph ~~5.5~~**5.6.** below”

*Annex 5, paragraph 7.1*., correct to read:

“7.1 The frequency, the "ON" time and the "OFF" time shall be as specified in the table below

|  |  | *Colour blue ~~or~~****,*** *amber* ***or red*** |
| --- | --- | --- |
|  |  | *rotating system or flash light sources*  *(Categories T and X)* |
| Frequency f (Hz) | max. | 4 |
| min. | 2 |
| "ON" time tH (s) | max. | 0.4/f |
| "OFF" time tD (s) | min. | 0.1 |

”

-----------------------------------------------