|  |  |  |
| --- | --- | --- |
|  |  | **INF.12** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Ninety-ninth session 5 November 2015**

Geneva, 9 – 13 November 2015

Item 6(b) of the provisional agenda

**Proposals for amendments to annexes A and B of ADR:**

**miscellaneous proposals**

References to standard EN 590:2009 + A1:2010

Transmitted by the Government of Germany

Introduction

In Chapter 3.2, Table A, in Table 4.1.1.21.6 and in paragraph 9.1.1.2 a) ADR in combination with UN 1202 a reference is made to an applicable standard EN 590:2009 + A1:2010.

The German delegation noticed, that a new version of this standard, i.e. **EN 590:2013 + AC:2014**, which came into force September 2013/March 2014 and replaced the previous version.

Proposal 1

Amend in **Table A, Chapter 3.2** ADR, the second entry for UN 1202 as follows:

|  |  |
| --- | --- |
| UN No. | Name and description |
|  | 3.1.2 |
| (1) | (2) |
| 1202 | DIESEL FUEL complying with standard EN 590:~~2009 + A1:2010~~2013 + AC:2014 or GAS OIL or HEATING OIL, LIGHT with a flash-point as specified in EN 590:~~2009 + A1:2010~~2013 + AC:2014 |

Proposal 2

Amend in **Table 4.1.1.21.6 Assimilation list** the entry “1202 Diesel fuel” as follows:

“

|  |  |  |
| --- | --- | --- |
| UN No. | Proper shipping name or technical name | Description |
|  | 3.1.2 | 3.1.2 |
| (1) | (2a) | (2b) |
| 1202 | **Diesel fuel** | complying with EN 590:~~2009 + A1:2010~~2013 + AC:2014 or with a flashpoint not more than 100 °C |

“.

Remark: the given description is not coherent with the description in Table A.

Proposal 3

Amend in **Table 4.1.1.21.6 Assimilation list** the entry “1202 Heating oil, light” as follows:

“

|  |  |  |
| --- | --- | --- |
| UN No. | Proper shipping name or technical name | Description |
|  | 3.1.2 | 3.1.2 |
| (1) | (2a) | (2b) |
| 1202 | **Heating oil, light** | complying with EN 590:~~2009 + A1:2010~~2013 + AC:2014 or with a flashpoint not more than 100 °C |

“.

Remark: the given description is not coherent with the description in Table A.

Proposal 4

Amend paragraph 9.1.1.2 a) as follows:

“(a) A vehicle intended for the carriage of liquids having a flash-point of not more than 60°C (with the exception of diesel fuel complying with standard EN 590:~~2009 + A1:2010~~2013 + AC:2014, gas oil, and heating oil (light) - UN No. 1202 - with a flash-point as specified in standard EN 590:~~2009 + A1:2010~~2013 + AC:2014) in fixed tanks or demountable tanks with a capacity exceeding 1 m3 or in tank-containers or portable tanks with an individual capacity exceeding 3 m3; or”.