|  |  |  |
| --- | --- | --- |
|  |  | **INF.26** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**100th session 9 May 2016**

Geneva, 9-13 May 2016

Item 5 of the provisional agenda

**Work of RID/ADR/ADN Joint Meeting**

 Amendment to 6.2.1.4

 Transmitted by the Government of France

 Introduction

1. Paragraph 18 of ECE/TRANS/WP.15/224 (report of the May 2014 session) reads:

«The Working Party noted that certain references to standards had been left in square brackets in informal document INF.5/Rev.1 because they were to be published in May or June 2014. The Working Party agreed to include these references as adopted texts (i.e. without square brackets) in ECE/TRANS/WP.15/222/Add.1. If the standards had not been published by 15 June 2014, the secretariat was requested to issue a corrigendum to ECE/TRANS/WP.15/222/Add.1 deleting these references.

*Note by the secretariat: the CEN secretariat informed the UNECE secretariat that standards EN ISO 14246:2014, EN ISO 10297:2014 and EN 12493:2013 + A1:2014 will not be published by 15 June 2014. Thus they are have not been included in the list of amendments for 2015.»*

2. The WG on Standards of the Joint Meeting proposed in March 2016 an additional amendment to EN 12493 so the reference to the last version of this standard appears in INF.3. But the amendments adopted in 2014 for EN ISO 14246 and EN ISO 10297 were forgotten and need to be added for entry into force on 1 January 2017.

 Proposal

3. In 6.2.4.1, Amend the Table, under "for closures", as follows:

– For standard "EN ISO 10297:2006", in column (4), replace "Until further notice" by "Between 1 January 2009 and 31 December 2018".

– After standard "EN ISO 10297:2006", insert the following new row:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN ISO 10297:2014 | Gas cylinders – Cylinder valves – Specification and type testing (ISO/DIS 10297:2012) | 6.2.3.1 and 6.2.3.3 | Until further notice |  |

– Add the following new row:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN ISO14246:2014 | Gas cylinders – Cylinder valves – Manufacturing tests and examinations (ISO 14246:2014) | 6.2.3.1 and 6.2.3.4 | Until further notice |  |