|  |  |  |
| --- | --- | --- |
|  |  | **INF.30** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods 14 September 2017**

Geneva, 19-29 September 2017

Item 2 of the provisional agenda

**Tanks**

Item 5 (b) of the provisional agenda

**Proposals for amendments to RID/ADR/ADN: new proposals**

Amendments to transitional measures

Note by the secretariat

The Joint Meeting may wish to consider the deletion or the modification of the following transitional measures in RID/ADR 2019.

Proposals

Amend the following transitional measures as shown:

**1.6.1 General**

1.6.1.1 Unless otherwise provided, the substances and articles of RID/ADR may be carried until 30 June 2019 in accordance with the requirements of ADR applicable up to 31 December 2018.

1.6.1.25 *(Deleted)*

1.6.1.39 *(Deleted)*

1.6.1.40 *(Deleted)*

1.6.1.41 Notwithstanding the requirements of ADR applicable as from 1 January 2017, large packagings conforming to the packing group III performance level in accordance with special packing provision L2 of packing instruction LP02 of 4.1.4.3 applicable until 31 December 2016 may continue to be used until 31 December 2022 for UN No. 1950.

1.6.1.42  *(Deleted)*

**1.6.3 Fixed tanks (tank-vehicles), demountable tanks and battery-vehicles**

1.6.3.16 *(Deleted)*

1.6.3.17  *(Deleted)*

1.6.3.42  *(Deleted)*

1.6.3.44 Fixed tanks (tank-vehicles) and demountable tanks intended for the carriage of UN Nos. 1202, 1203, 1223, 3475 and aviation fuel classified under UN Nos. 1268 or 1863, equipped with additive devices designed and constructed before 1 July 2015 in accordance with national provisions, but which do not, however, conform to the construction, approval and testing requirements of special provision 664 of Chapter 3.3 applicable as from 1 January 2015, shall only be used with the agreement of the competent authorities in the countries of use.

**1.6.4 Tank-containers, portable tanks and MEGCs**

1.6.4.15  *(Deleted)*

1.6.4.18  *(Deleted)*

1.6.4.38 *(Deleted)*

1.6.4.44 *(Deleted)*

1.6.4.45 *(Deleted)*