UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/811
3 August 2001

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

CORRIGENDUM 1 TO SUPPLEMENT 3 TO THE 03 SERIES

OF AMENDMENTS TO REGULATION No. 36

(Large passenger vehicles)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its eighteenth session, following the recommendation by WP.29 at its one-hundred-and-twenty-fourth session. It is based on document TRANS/WP.29/2001/13, not amended (TRANS/WP.29/792, para. 152).

__________

Paragraph 5.6.4.9., correct to read (English and Russian only):

"5.6.4.9.	The service door in any open position shall not obstruct the use of, or required access to any mandatory exit."

__________

GE.01-