UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/812
3 August 2001

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 3 TO THE 01 SERIES

OF AMENDMENTS TO REGULATION No. 52

(Small passenger vehicles, M2 and M3 category)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its eighteenth session, following the recommendation by WP.29 at its one-hundred-and-twenty-fourth session. It is based on document TRANS/WP.29/2000/52, not amended (TRANS/WP.29/792, para. 154).

__________

Paragraph 5.7.1.12., amend to read:

"5.7.1.12.	The maximum slope of the floor in the access passage shall not exceed 5 per cent."

____________

GE.01-