|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.11/2016/11 |
| _unlogo | **Economic and Social Council** | Distr.: General19 July 2016EnglishOriginal: Russian |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Perishable Foodstuffs**

**Seventy-second session**

Geneva, 4-7 October 2016

Item 5 (b) of the provisional agenda

**Proposals of amendments to ATP: New proposals**

 Editorial correction to Russian-language version of ATP

 Transmitted by the Government of the Russian Federation

|  |
| --- |
|  *Summary* |
| **Executive summary**: When working with the text of ATP, in Section 2 of Model No. 2 A of the test reports contained in Appendix 2 of Annex 1 to ATP, an error was identified in the formula for the K coefficient for the inside-heating test.  In the Russian-language version the formula is given as K $=\frac{W\_{1}-W\_{2}}{S.∆T} $ However, the English and French-language versions have the correct formula for the K coefficient K $=\frac{W\_{1}+W\_{2}}{S.∆T}$ |
| **Action to be taken:** Introduce the editorial correction to the Russian-language version in Section 2 of Model No. 2 A in Appendix 2 of Annex 1 to ATP , by giving the correct formula for the K coefficient for the inside-heating test K $=\frac{W\_{1}+W\_{2}}{S.∆T}$ |
| **Background**: None |
|  |